### Resonant Filter

VCF with LFO and EG

Freq | Cut-off frequency
Rez | Resonance
Output | Level trim
Env->VCF | Positive or negative (squelchy!) Envelope modulation of cut-off frequency
Attack |
Release | (use fast attack and release for "dirty" modulation)
LFO->VCF | LFO modulation of cut-off frequency (turn to left for sample & hold LFO, right for sine)
LFO Rate | LFO modulation speed
Trigger | Envelope trigger level (normally set to minimum to acts as a free-running envelope follower)
Max Freq | Limit maximum cut-off frequency for a mellower sound (the filter can sound "screechy" at high frequencies)