### Stereo Simulator

Add artificial width to a mono signal

Width | Stereo width (turn to right for comb filter mode, left for Haas panning mode)
Delay | Delay time - use higher values for more filter "combs" across the frequency spectrum
Balance | Balance correction for Haas mode
Mod | Amount of delay modulation (defaults to OFF to reduce processor usage)
Rate | Modulation rate (note that modulation completely disappears in mono)

This plug converts a mono signal to a ' wide' signal using two techniques: Comb filtering where the signal is panned left and right alternately with increasing frequency, and Haas panning where a time delayed signal sounds appears to be at the same level as a quieter non-delayed version.

Comb mode is mono compatible. Haas mode is not, but sounds fine on some signals such as backing vocals. This plug-in must be used in a stereo channel or bus!

###

###