### Image

Stereo image adjuster and MS matrix

Allows the level and pan of mono and stereo components to be adjusted separately, or components to be separated for individual processing before recombining with a second Image plug-in.

Mode | LR->LR - stereo image adjustment LR->MS - encode to MS MS->LR - decode from MS SM->LR - decode from MS (input channels reversed)
S Width | Stereo width (level of stereo component)
S Pan | Stereo image "skew"
M Level | Centre "depth"
M Pan | Centre pan
Output | Level trim (a 6dB correction may be required for some MS encoded material)

###

###