### Thru-Zero Flanger

Tape flanger and ADT

This plug simulates tape-flanging, where two copies of a signal cancel out completely as the tapes pass each other. It can also be used for other "modulated delay" effects such as phasing and simple chorusing.

Rate | Modulation rate (sine wave) - set to minimum for static comb filtering
Depth | Maximum modulation depth
Mix | Wet / dry mix - set to 50% for complete cancelling
Feedback | Add positive or negative feedback for harsher or "ringing" sound
Depth Mod | Modulation depth - set to less than 100% to limit build up of low fequencies with feedback

###