### Test-Tone Generator

Mode |
MIDI # IMPULSE WHITE PINK SINE LOG SWP LOG STEP LIN SWP | - sine waves at musical pitches (A3 = 69 = 440 Hz) - single-sample impulse - white noise - pink noise - ISO 1/3-octave frequencies - logarithmic frequency sweep - 1/3-octave steps - linear frequency sweep
Level | Peak output level
Channel | Generate signals on left or right channel only
F1 | Base frequency (not applicable to pink and white noise or impulses)
F2 | Fine frequency control, or end frequency for sweep modes
Sweep | Sweep duration for sweep modes (2 seconds silence is also added between sweeps) Sets repetition rate in inpulse mode
Thru | Allow the input signal to pass through the plug-in
0 dB = | Calibrate output so indicated level is relative to, for example -0.01 dB FS or -18 dB FS

For more extensive test and measurement try WaveTools (http://www.maxim.abel.co.uk)

###