mai | JUIN | juil.
| 30 |
2007 | 2008 | 2009
1 captures 30 juin 08 - 30 juin 08 |
| Close Help

:: Home :: FAQ :: Search :: Memberlist :: Usergroups :: Register :: Profile :: Log in to check your private messages :: Log in ::

[Q] Silence? of an instrument
| Skale Tracker Forum Index -> Documentation, Tips & Tricks
View previous topic :: View next topic
Author | Message
--- | ---
Blacker Skale Clueless Joined: 16 Nov 2005 Posts: 4 Location: Sweden |
Posted: Wed Nov 16, 2005 3:43 pm Post subject: [Q] Silence? of an instrument |
Hi, I'm quite new on this and I was wondering how to have an instrument silent? Let's say I have two patterns, 1 and 2 following eachother, then I would like to have pattern 1 played again after that. Problem is that an instrument from pattern 2 still plays and overlaps pattern 1. So how do I get pattern 2 silent?
Back to top |
vereiser Skale Moderator Joined: 04 Nov 2004 Posts: 314 Location: Berlin, Germany |
Posted: Thu Nov 17, 2005 3:37 am Post subject: |
three possibilities you have: 1. hard (sample only): use the volume command in the track editor (switch pattern effetcs to get it) and set the effect to 0 2. soft (sample, vsti): - set a volume envelope curve to the instrument (Instr.Ed.) - set a fade out other than 0 (Instr.Ed.) - use the substain command (note off, could be setted in ConfigSkale.Exe->Shortcuts) to stop the instrument with the fade out you've setted 3. static (sample) use the volume envelope of the instrument and fade out the instrument bwith an envelope curve _________________ http://www.vereiser.de Intel Pentium 4 / 2,8 GHz / 1 GB DDR / WinXP Prof. / Hoontech DSP24 Value (multichannel soundcard) Last edited by vereiser on Fri Nov 18, 2005 9:17 pm; edited 2 times in total
Back to top |
st3vie Skale Administrator Joined: 13 Nov 2002 Posts: 641 Location: Beverwijk, The Netherlands |
Posted: Thu Nov 17, 2005 6:55 am Post subject: |
*moved to Docs, Tips & Tricks*
Back to top |
Blacker Skale Clueless Joined: 16 Nov 2005 Posts: 4 Location: Sweden |
Posted: Thu Nov 17, 2005 2:31 pm Post subject: |
Thanks. I've used the volume command in the track editor and that worked fine.
Back to top |
vereiser Skale Moderator Joined: 04 Nov 2004 Posts: 314 Location: Berlin, Germany |
Posted: Fri Nov 18, 2005 9:15 pm Post subject: |
But the soft method will be the professional one at least. _________________ http://www.vereiser.de Intel Pentium 4 / 2,8 GHz / 1 GB DDR / WinXP Prof. / Hoontech DSP24 Value (multichannel soundcard)
Back to top |
Blacker Skale Clueless Joined: 16 Nov 2005 Posts: 4 Location: Sweden |
Posted: Sat Nov 19, 2005 7:58 pm Post subject: |
Quote:
But the soft method will be the professional one at least.
OK. I'm not sure how to really do this though.
Back to top |
Display posts from previous:
| Skale Tracker Forum Index -> Documentation, Tips & Tricks | All times are GMT + 1 Hour
Page 1 of 1
Jump to:
You cannot post new topics in this forum You cannot reply to topics in this forum You cannot edit your posts in this forum You cannot delete your posts in this forum You cannot vote in polls in this forum
Powered by phpBB © 2001, 2005 phpBB Group