### VocInput

Vocoder carrier signal

This plug-in produces a voice-like signal on the right channel to be used as a carrier signal with vocoder and other vocoder plug-ins. The input signal passes through on the left channel.

Tracking |
OFF FREE QUANT | - Constant pitch - Track input pitch - Track input pitch to nearest semitone
Pitch | Oscillator pitch, or pitch transpose in tracking modes
Breath | Amount of breath noise
S Thresh | Sensitivity for adding sibilance / fricative noise to consonants
Max Freq | Maximum allowed pitch - mainly used to reduce pitch tracking errors

###