### Multi-Band Compressor

Three-band soft-knee compressor with switchable M or S component processing

As well as just "squashing everything" this plug-in can be used to "overcook" the mid-frequencies while leaving the low end unprocessed, enhancing playback over small speakers without affecting the overall sound too much.

Listen | Audition the low, mid and high bands individually
L <> M | Low / mid crossover frequency
M <> H | Mid / high crossover frequency
L/M/H Comp | Compression amount for each of the 3 bands
L/M/H Out | Output level trims (for spectrum shaping - make-up gain is applied automatically)
Attack |
Release |
Stereo Width | Used to restore stereo width when heavy processing is applied to Mono component
Process | Select Mono or Stereo component

To give more control when mastering (and to offer something different from other dynamics processors) in Mono mode this plug does not compress any stereo information, but in Stereo mode only the stereo component is processed giving control over ambience and space with a similar sound to strereo "shufflers" - but be careful with the levels! The stereo width control works as a "mono depth" control in Stereo mode.

###

###